     *    *  * * *  *     *  * * * * *  * * *      *     *    *  *   * * *
     * *  *  *      *     *      *      *    *   *   *   * *  *  *   *
     *  * *  * *    *  *  *      *      * * *   *     *  *  * *  *   *
     *   *   *      * * * *      *      *   *    *   *   *   *   *   *
     *    *  * * *   *   *       *      *    *     *     *    *  *   * * *
     

                               N E W T R O N I C

                       Sound Design & Midi Software Ltd.

                        62b Manor Avenue London SE4 1TE

                Tel 0181 691 1087        Int +44 181 691 1087
                Fax 0181 691 2284        Int +44 181 691 2284


                             (c) NEWTRONIC 1996


Newtronic 
Pro Studio Loops

MIDI Gates, Pans & Fades



Congratulations on purchasing this collection of midi gate, pan
and fade templates. There are over a hundred different files containing
varied MIDI controller data saved as Standard MIDIFILE Format (SMF).

The files can be easily loaded into your sequencing software. Most 
templates measure 1 bar. You should copy them on to make them as long
as you wish. 

All templates are programmed on MIDI Channel 1. To hear the effect of
the controller data you must select a long sound (pad, synth or string)
on Channel 1 play it while the sequencer is in running mode.


The files are split into easily recognisable groups:



Files with the prefix :   acc-accented gates 

	b- basic gates

	fade- fade outs of 1,2, and 4 bars

	fd-d-u(number)- fade down then up over number of bars

	fd-up(number)- fade up over number of bars
  
	long- gates which are open for longer providing a smoother
	sound

  pan(number)l-r- pan in 16th/12th notes etc. from left to right

	panhrd(number)- hard panning from extreme to extreme

	random- 4 bar random gate effects

	rhythm- rhythmic groove gates

	shuffle(number)- shuffle gate in 16th/12th notes etc.

	slowup- gates that start fast and slow down over time

	speedup- opposite to above

	v(number)inarow- (number) of 16th notes in a row, with a 16th
	note gap


User Notes:


Each gate has a main volume=127 event in the last bar so that
sounds are not left at 0 volume. If you want to extend the
length of the gate bars simply cut off the last bar and repeat
the gate bars as normal

Each pan bar has a reset value of pan=64 (centre position) in
the last bar. If you want to extend the length of the pan bars
simply cut off the last bar and repeat as normal.

We choose to select Volume (controller 7) instead of Expression
because it is also recognized by older MIDI gear. If you prefer
the more "stylish" Expression data simply use the global convert
function in your sequencer. 



Enyjoy working with this product and don't forget to look out for
new releases in the Pro Studio Loops series.


NEWTRONIC Team (1996)


Copyright - Don't Pirate

Pro Studio Loops - MIDI Gates, Pans & Fades are subject to copyright.
The software is licenced to the user under standard software licencing
agreement. No hiring, copying, re-sale etc. Any copyright infringement
will be prosecuted to the fullest extent the law permits. 

